**Step 3.4: Pseudo Code**

IF IGN = HIGH THEN

IF (DRIV = HIGH AND BELTD = LOW) OR (PASS = HIGH AND BELTP = LOW) THEN

ALARM = LOW // Alarm ON

ELSE

ALARM = HIGH // Alarm OFF

ENDIF

ELSE

ALARM = HIGH // Alarm OFF (ignition off)

ENDIF